|  |  |  |
| --- | --- | --- |
| TYPE | UNITS | SPEC  |
| 1 TB USB HDD for backup storage | 1 | 1TB Near Line SAS 6Gbps 7.2k 3.5" HD Hot Plug Fully Assembled - Kit |
| Server Spec information | 1 | Dell PowerEdge R720 324,216.00Risers with up to 6, x8 P Cle Slots + 1, x16 P Cle SlotBezelReady Rails Sliding Rails with cable Management Arm3.5 “ Chassis with up to 8 Hard DrivesDeclined Remote AdvisoryiDRAC7 EnterpriseBroadcom 5720 QP 1Gb Network Daughter CardPower Saving Dell Active Power ControllerIntel Xeon E5-2609 2.40GHz, 10M Cache, 6.4GT/s QPI, No Turbo, 4C, 8oW,DDR3-1066MHzNo Additional Processor(2) 4GB RDIMM, 1333 MHZ, Low Volt, Dual Rank, x81333 MHZ RDIMMs(2) 500GB, SATA, 3.5-in, 7.2K RPM Hard Drive (Hot-Plug)16X DVD+/-RW, SATA InternalC2-RAID 0 for H710p/H710/H310,1-16 HDDs, Max base on the ChassisPERC H710 integrated RAID controller, 512MB NV Cacheperformance OptimizedSingle, Hot -Plug Power Supply (1+0), 750WRack Power Cord 2M (C13/C14 12A)3 Yr. Basic Warranty |
| WinSBSEssntls 2008 SNGL OLP NL QlfdUpto 25 users | 1 |  |
| SQL Server STD 2008 (Should be able to upgrade to higher version if necessary) | 1 |  |
| 5 Clients (with SQL-2008) | 5 |  |
| The SonicWALL® TZ 200 Series -1 year total security integrates Unified Threat Management with critical business continuity features to provide a powerful branch office and small business security platform(option) | 1 |  |
| ESET NOD32 Antivirus Business Edition for 1 year | 20 |  |
| 27U 800 x 800 Sever Rack - For Server | 1 |  |
| Data backup for Head office-Symantec System Recovery for Server 2012 Standard (option) | 1 |  |
| MGE 3000V A UPS for server power protection | 1 |  |
| Dlink Gigabit Switch - 24 Port (option) | 1 |  |